(footprint "1MS1T1B4M7QES" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at -2.5 -1 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6f19263d-9d66-4b2e-80b1-24aade278735)
  )
  (fp_text value "1MS1T1B4M7QES" (at 2.5 -5 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp de16042a-7dae-4f9c-9d26-2f93e3160ef5)
  )
  (fp_text user "${REFERENCE}" (at -2.5 -1 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b5b4c637-1f74-4c91-92f3-b635f0ce12cb)
  )
  (fp_line (start -3.5 3.18) (end 3.5 3.18)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9e138a13-d287-4964-aa51-2fbaa7ecc428))
  (fp_line (start -3.5 11.5) (end -3.5 3.18)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e8866983-23af-47a0-a868-e46bb109332b))
  (fp_line (start 3.5 3.18) (end 3.5 11.5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e6a90364-2b54-49bc-a816-b9bc7e9bbec6))
  (fp_line (start -3.11 20) (end -3.11 12.7)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp c00beb2b-102c-4f7a-9aab-9fbff2701219))
  (fp_line (start -1.34 20) (end -1.34 26.46)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp 1ea62593-9783-40e7-99b4-60ec43132319))
  (fp_line (start -1.34 26.46) (end 1.34 26.46)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp b0e3cd34-5e6b-48e7-a6f7-4e008e199889))
  (fp_line (start 1.34 26.46) (end 1.34 20)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp aedc63b1-1f89-4d99-9080-452236d8d1ef))
  (fp_line (start 3.11 12.7) (end 3.11 20)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp fe2dc5b5-ef1a-4d83-8e75-0800101020dc))
  (fp_line (start 3.11 20) (end -3.11 20)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp 6b255460-ffeb-43cd-b251-1f1d396833c3))
  (fp_line (start -4 1.5) (end -4 14.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8e23c522-7df1-4ead-88db-fb2d2d12d936))
  (fp_line (start -4 14.25) (end 4 14.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 76e3d991-ef31-418c-9b20-139052ed4faa))
  (fp_line (start -1.5 -9.25) (end -1.5 1.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6998c619-00d6-4194-89c4-5180a9295fc0))
  (fp_line (start -1.5 1.5) (end -4 1.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 01df2f93-1c9d-4601-962d-1d9ccdb9be24))
  (fp_line (start 1.5 -9.25) (end -1.5 -9.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 38a7ce3f-a7bd-44ca-85de-c7cc12d2cc2e))
  (fp_line (start 1.5 1.5) (end 1.5 -9.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2a826a4f-e234-4aa7-9813-6a066706c4ba))
  (fp_line (start 4 1.5) (end 1.5 1.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7067faea-234e-4f42-a9f1-824292f29ded))
  (fp_line (start 4 14.25) (end 4 1.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp afac944f-f388-4487-aee7-39ab69928e1b))
  (fp_rect (start -3.43 12.7) (end 3.43 3.25)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 6e264ce3-928b-4aaf-8a5e-54b2a105d94a))
  (pad "1" thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp ef3e7ee8-18b8-4170-b8d9-98bc7eb6a3a2))
  (pad "2" thru_hole circle (at 0 -3.81) (size 2.8 2.8) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp a37571b4-cb53-48fd-86b1-2e7335d990f0))
  (pad "3" thru_hole circle (at -0.009442 -7.62) (size 2.8 2.8) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp f0ee6f72-adfe-49ad-ad1d-0f9be74506b9))
  (pad "S" thru_hole circle (at -2.54 12.7) (size 2.8 2.8) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp a49ef391-5290-491f-b571-2712c7f250a0))
  (pad "S" thru_hole circle (at 2.54 12.7) (size 2.8 2.8) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 607c4361-c515-4b30-b3cd-d740fdacf451))
  (model "${LORA_WINDPOWER_CONTROL}/Library/Models.3D/TE_A101SYAV2B04.wrl"
    (offset (xyz 0 -12.4 6.32))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
