(footprint "Schurter_31.3981" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 4.8 -7.75 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0542e343-199f-4d66-a7f2-a0e9805f65e3)
  )
  (fp_text value "Schurter_31.3981" (at 11.6 7.6 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bbfce1b3-3f52-4d21-9cef-ff5aff42a30a)
  )
  (fp_line (start 24.08 -6.66) (end -7.1 -6.66)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 3ca99ed9-38ca-4c16-9d6f-baf3b65a9973))
  (fp_line (start 24.08 -6.66) (end 24.08 6.66)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 2791990e-c3b5-4261-8579-58214c0fd074))
  (fp_line (start 24.08 6.66) (end -7.1 6.66)
    (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp f67abbb6-2f26-41bd-96b5-f247e6b723cb))
  (fp_circle (center 0 -5.715) (end 0.65 -5.715)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.Mask") (tstamp e4e5364c-c010-4fae-bec8-7059b7919679))
  (fp_circle (center 0 5.715) (end 0.65 5.715)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.Mask") (tstamp 22158d43-3772-407e-a4b3-09d338fa915a))
  (fp_line (start -11.18 -6.5) (end -11.18 6.5)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp d306b7dc-c05a-4478-8caa-27a4032468a6))
  (fp_line (start -11.18 6.5) (end -7.2 6.5)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp e4f39c99-c8d8-4f29-a5aa-b5290566fd2d))
  (fp_line (start -7.2 6.5) (end -7.18 -6.5)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp b1e5062c-5c40-44b5-beaf-4952fc5245a3))
  (fp_line (start -7.18 -6.5) (end -11.18 -6.5)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp 0add63ab-d24f-49a5-ae34-c59a1cb93291))
  (fp_line (start -7.18 -6.65) (end -7.18 6.65)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c8400179-32dd-4441-9fc7-451afc5278f9))
  (fp_line (start -7.18 6.65) (end 24.1 6.65)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1292320a-9c82-4bb8-875d-878a70eac264))
  (fp_line (start 24.1 -6.65) (end -7.18 -6.65)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3faec127-7ad2-4740-b76a-828d5af04129))
  (fp_line (start 24.1 6.65) (end 24.1 -6.65)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 564be989-c331-494f-af80-7519a251c4c5))
  (fp_line (start -7.18 -6.5) (end -7.18 6.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1f848fb3-6db7-4662-bc6e-d396bea24010))
  (fp_line (start -7.18 -6.5) (end 23.92 -6.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3c62069d-d69b-4456-b3f1-b4d6a572e494))
  (fp_line (start -7.18 6.5) (end 23.92 6.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c2ce242c-4323-4121-958c-ba1dee6a67dc))
  (fp_line (start 23.92 -6.5) (end 23.92 6.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2fccd89e-3da0-4e50-b644-02d5dccc5c21))
  (pad "" np_thru_hole oval (at 0 -5.715) (size 2.5 1.6) (drill 1.3) (layers "B.Cu" "B.Mask")
    (clearance 0.2) (tstamp 25dc1305-7874-4cc2-9a77-f819d5cbc5e8))
  (pad "" np_thru_hole oval (at 0 5.715) (size 2.5 1.6) (drill 1.3) (layers "B.Cu" "B.Mask")
    (clearance 0.2) (tstamp f335479f-c26d-4570-b486-ea2bf036123b))
  (pad "1" thru_hole rect (at 20.32 -4.45) (size 2.5 1.6) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp 7d43dcdb-f070-42a4-9981-ec8c9cdf8de0))
  (pad "2" thru_hole oval (at 20.32 4.45) (size 2.5 1.6) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp 2f5a9440-8fd3-441d-962b-8cf7050fba15))
  (model "${LORA_WINDPOWER_CONTROL}/Library/Models.3D/Schurter_31.3981.step"
    (offset (xyz -7.17 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 90))
  )
)
