(footprint "Keystone_5001" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "solder Pin_ diameter 2.54mm, hole diameter 1.0mm (press fit), length 7.62mm")
  (tags "solder Pin_ press fit")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 2.25) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp aa873d6e-828f-47d9-8564-a7b1bd2e5933)
  )
  (fp_text value "Keystone_5001" (at 0 -2.05) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fc162139-c967-4d0c-a998-335b182d6df2)
  )
  (fp_text user "${REFERENCE}" (at 0 2.25) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f063d92e-58ec-461d-ab96-69d05bb299b7)
  )
  (fp_circle (center 0 0) (end 1.27 0.0762)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp a8d3515a-ce0a-4721-9112-032fd8a53f30))
  (fp_circle (center 0 0) (end 1.3716 0.0254)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 1e3d2eab-2b89-4079-a2e4-2fb0e8aff0ae))
  (fp_circle (center 0 0) (end 0.5 0)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.Fab") (tstamp a802bc52-407f-4402-b3d5-ac10e6813818))
  (fp_circle (center 0 0) (end 1 0)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.Fab") (tstamp 6e29884d-bf0f-41ab-ab00-f03e7e67ce7f))
  (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 10ce94dd-fbea-4164-a68f-fbb193f565d7))
  (model "${LORA_WINDPOWER_CONTROL}/Library/Models.3D/Keystone 5001.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
