(footprint "Converter_DCDC_TRACO_THN30-xxxx_THT" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "DCDC-Converter TRACO THN 10 to 30W, Single or dual Output, (https://www.tracopower.com/sites/default/files/products/datasheets/thn30_datasheet.pdf)")
  (tags "DCDC-Converter TRACO THN30 Generic")
  (attr through_hole)
  (fp_text reference "REF**" (at 5.08 -3.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1018289e-49ed-4f59-9a54-aa3138a3fb1d)
  )
  (fp_text value "Converter_DCDC_TRACO_THN30-xxxx_THT" (at 2.54 24 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 15aeb366-43f8-436f-b629-c342b5f83745)
  )
  (fp_text user "${REFERENCE}" (at 2.54 10.16 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 37350984-deba-466b-8114-b3a370ff7948)
  )
  (fp_line (start -10.31 -2.69) (end -10.31 22.93)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 02d0954c-49c9-4a2d-a5c0-727a89d8f184))
  (fp_line (start -10.31 -2.69) (end 15.31 -2.69)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp f6bb94ae-f7a5-428b-a71d-50d851cda5b9))
  (fp_line (start -10.31 22.93) (end 15.31 22.93)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp acc1f7f2-a91e-4a50-94e9-ed9d9aa2d490))
  (fp_line (start -1.2 -3) (end 1.2 -3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 7f6ca0ff-a64b-427d-b1e1-8582113a95cf))
  (fp_line (start 15.31 22.93) (end 15.31 -2.69)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 5063ae78-2427-4660-84bf-6e0f1ff1a85b))
  (fp_line (start -10.45 -2.83) (end -10.45 23.07)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3e68cab8-446a-497d-973a-a06aaa00c578))
  (fp_line (start -10.45 -2.83) (end 15.45 -2.83)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 26d7bef2-aa52-407a-918b-a83acf54493c))
  (fp_line (start -10.45 23.07) (end 15.45 23.07)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 56857d74-8c38-4da6-aadc-08e1344c0104))
  (fp_line (start 15.45 -2.83) (end 15.45 23.07)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 68c67c81-f7e0-472f-ba27-7967998309ea))
  (fp_line (start -10.2 -2.58) (end -10.2 22.82)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 1fcb180b-0203-42a6-8932-f0450d028313))
  (fp_line (start -10.2 -2.58) (end -1 -2.58)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 0bfa6624-84a0-4728-9f9f-056dc2921a3d))
  (fp_line (start -10.2 22.82) (end 15.2 22.82)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 3f5f62d4-d24a-405a-9e95-598ce6e9f1ad))
  (fp_line (start -1 -2.58) (end 0 -1.58)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 938af59b-3004-429e-9abf-bdfa1268372f))
  (fp_line (start 1 -2.58) (end 0 -1.58)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 92636165-6f51-4e27-bc54-e5460559e085))
  (fp_line (start 1 -2.58) (end 15.2 -2.58)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp c30650ab-7429-459b-a809-7e5cd22fe932))
  (fp_line (start 15.2 -2.58) (end 15.2 22.82)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 569deefb-1027-4aa6-a9ac-0ddbcef37d8d))
  (pad "1" thru_hole roundrect (at 0 0) (size 2 2) (drill 1.24) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp b31fd0b4-bb30-43ce-b76a-c13e0dfe2f60))
  (pad "2" thru_hole circle (at 5.08 0) (size 2 2) (drill 1.24) (layers "*.Cu" "*.Mask") (tstamp 2eb9c803-bd4f-4bf9-b5cd-0c3050f48fe3))
  (pad "3" thru_hole circle (at -7.62 20.32) (size 2 2) (drill 1.24) (layers "*.Cu" "*.Mask") (tstamp 55de05f6-5848-49de-a2ea-6adf9f982935))
  (pad "4" thru_hole circle (at 2.54 20.32) (size 2 2) (drill 1.24) (layers "*.Cu" "*.Mask") (tstamp 23891bf7-4b1c-419f-869e-fc8ef8bcf2f8))
  (pad "5" thru_hole circle (at 12.7 20.32) (size 2 2) (drill 1.24) (layers "*.Cu" "*.Mask") (tstamp 686ea1f4-ca67-4043-ac3a-2a633d0d7139))
  (pad "6" thru_hole circle (at 12.7 0) (size 2 2) (drill 1.24) (layers "*.Cu" "*.Mask") (tstamp 3471c8c6-52bc-4714-ae2b-05936fbe12ff))
  (model ":LORA_WINDPOWER_CONTROL:Library/Models.3D/CUI_PDQE20-Q24-D5-D.step"
    (offset (xyz 2.54 -10.2 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
