(footprint "LED_Bi-Color_3225_K13" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at -0.45 -2.35 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dc1d338c-9979-48e7-b84b-53d5bc23cc7c)
  )
  (fp_text value "LED_Bi-Color_3225" (at 0 2.45 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 61c01823-cee0-4843-a846-f5550eef3ae2)
  )
  (fp_text user "${REFERENCE}" (at -0.45 -2.35 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp df153fb0-7fa0-4626-874e-1fd75166cb5e)
  )
  (fp_line (start -2.35 1.45) (end -2.35 -1.45) (layer "F.SilkS") (width 0.12) (tstamp 2c8fc146-f6c2-47bb-ba53-d50686f9b6ad))
  (fp_line (start 2.35 1.45) (end -2.35 1.45) (layer "F.SilkS") (width 0.12) (tstamp 75128e1b-2530-4e60-96f9-4af5af708dd0))
  (fp_line (start -2.35 -1.45) (end 2.35 -1.45) (layer "F.SilkS") (width 0.12) (tstamp 7c1a151c-ceba-4fcc-a392-d8643296f5c0))
  (fp_line (start 2.35 -1.45) (end -2.35 -1.45) (layer "F.CrtYd") (width 0.05) (tstamp 12a71947-bfbd-4966-8fe9-16fbfdc6c776))
  (fp_line (start 2.35 1.45) (end 2.35 -1.45) (layer "F.CrtYd") (width 0.05) (tstamp 4daec474-c89f-4a1d-b613-d530b7df8d81))
  (fp_line (start -2.35 1.45) (end 2.35 1.45) (layer "F.CrtYd") (width 0.05) (tstamp 7b4b2c2f-290a-4844-8e67-e0cc77420539))
  (fp_line (start -2.35 -1.45) (end -2.35 1.45) (layer "F.CrtYd") (width 0.05) (tstamp d1a28ae8-5fdf-421e-9f96-5743d655755b))
  (fp_rect (start -1.6 -1.35) (end 1.6 1.35) (layer "F.Fab") (width 0.1) (fill none) (tstamp 4deee43e-5acf-447d-91a7-114d94fb0e2f))
  (pad "1" smd roundrect (at -1.35 -0.775) (size 1.7 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 351ac680-c5fa-4c71-ba80-456348673995))
  (pad "2" smd roundrect (at 1.35 -0.775) (size 1.7 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 84280b38-c71d-49bc-b03f-678b8ee02f3d))
  (pad "3" smd roundrect (at -1.35 0.775) (size 1.7 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7f53d358-822f-4c41-a346-b5c27feddb91))
  (pad "4" smd roundrect (at 1.35 0.775) (size 1.7 1.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d0abb871-8ddc-435c-83c5-03b09be37358))
  (model "${ACCELEROMETER_PCB}/Models.3D/LED_Bi-Color_3225.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
