(footprint "Antenna-Mount" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 7.62 -4.826 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 174e6c78-30f2-4983-8860-b0dba65e9394)
  )
  (fp_text value "Antenna-Mount" (at 0 -7.366 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3e0276cd-88ff-45cd-b818-380445e60caa)
  )
  (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 944bd18e-6e68-42eb-9020-b9a2b41ca5d7)
  )
  (fp_circle (center 0 0) (end 6.3 0)
    (stroke (width 0.15) (type default)) (fill none) (layer "F.SilkS") (tstamp 69cc91c1-b5cf-43e3-bfe6-63f34d887c9d))
  (fp_circle (center 0 0) (end 3.3 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 9f3daae9-f119-4b00-b95f-d19b35b8e526))
  (pad "" np_thru_hole circle (at 0 0) (size 6.5 6.5) (drill 6.5) (layers "F&B.Cu" "*.Mask")
    (clearance 3) (tstamp 6ece17d2-91e5-41a7-aa96-15f895277f48))
  (model ":LORA_WINDPOWER_CONTROL:Library/Models.3D/SMA_Jack.step"
    (offset (xyz -1.5 -2.5 1.5))
    (scale (xyz 1 1 1))
    (rotate (xyz -45 6 0))
  )
  (model ":LORA_WINDPOWER_CONTROL:Library/Models.3D/SMA_Antenna.step"
    (offset (xyz 0 -5 28.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
