(footprint "ZFKDSA 1,5-W-5,08-2" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at -2.794 -3.556 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 350285e6-5235-405f-ae0d-5c4b25ddfac9)
  )
  (fp_text value "ZFKDSA 1,5-W-5,08-2" (at 3.81 11.43 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a2c84add-d530-456c-956e-66ba247f2f13)
  )
  (fp_text user "${REFERENCE}" (at 2.794 13.208 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2511b095-c038-4e16-a1fe-ecc81ed85cac)
  )
  (fp_line (start -4.75 -2.64) (end -4.75 10.26)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 4876c43b-692b-4720-91ee-42bfa1f208bb))
  (fp_line (start -4.75 -2.64) (end 12.3 -2.64)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 69d40496-d1da-4185-af8e-bfc99c3d581e))
  (fp_line (start -4.75 10.26) (end 12.3 10.26)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp d03b2a47-ebbd-4ca5-b027-400247942ac4))
  (fp_line (start 12.3 -2.64) (end 12.3 10.26)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 76d86453-ddd6-4dd8-b61d-75c7426a428a))
  (fp_line (start -4.95 -2.84) (end -4.95 10.46)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp df7a2491-a732-435a-9792-e797888356c4))
  (fp_line (start -4.95 -2.84) (end 12.5 -2.84)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5478c83f-2dcf-4bcb-a06a-a11a4e0ded38))
  (fp_line (start -4.95 10.46) (end 12.5 10.46)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9324ad82-394c-4165-9e5d-c570efed6797))
  (fp_line (start 12.5 -2.84) (end 12.5 10.46)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fc49f408-4493-4e33-9fc6-6da02c1dcc4a))
  (fp_line (start -4.65 -2.54) (end -4.65 10.16)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 32261f00-9ac1-4094-8788-4662ff565904))
  (fp_line (start -4.65 -2.54) (end 12.2 -2.54)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 4a2ed3f0-be7d-45c0-94e9-5f074d073c6e))
  (fp_line (start -4.65 10.16) (end 12.2 10.16)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 58bf7c51-160f-4801-af76-fc2735672ac1))
  (fp_line (start 12.2 -2.54) (end 12.2 10.16)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp d4706bed-5d3f-4382-ade8-9040613e7997))
  (pad "1" thru_hole oval (at 0 0) (size 3 2) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp f811c908-b8f9-4768-b011-2931fdcccc23))
  (pad "1" thru_hole oval (at 5.08 0) (size 3 2) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp b761beec-945c-4502-b64c-dee5131e4eb2))
  (pad "2" thru_hole oval (at 0 5.08) (size 3 2) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp 93981e10-7e39-48a6-98ad-1ff3d96b6c21))
  (pad "2" thru_hole oval (at 5.08 5.08) (size 3 2) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp f62a6f97-8e1d-476a-8ef7-5d9adfad0593))
  (model ":LORA_WINDPOWER_CONTROL:Library/Models.3D/PhoenixContact_ZFKDSA-1-5-W-5-08-2_3D.stp"
    (offset (xyz -3.27 -10.15 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
