(footprint "Case_1455T1201" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr exclude_from_pos_files)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "Dwgs.User")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c511ee60-efdf-4d0d-9bc7-e57147ab1691)
  )
  (fp_text value "Case_1455T1201" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bc447ad3-7cde-4901-9abe-90c57c7d9267)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 504f9bce-d1cf-4eea-a145-946eb65c812f)
  )
  (fp_line (start -59.95 73.35) (end 59.95 73.35) (layer "B.SilkS") (width 0.09) (tstamp 209d2740-f8e8-4175-8bcc-d34fa0267f2b))
  (fp_line (start -59.95 -73.35) (end 59.95 -73.35) (layer "B.SilkS") (width 0.09) (tstamp 456fa5d8-2cd4-4af3-b497-42c98effaed0))
  (fp_line (start -59.95 77.35) (end 59.95 77.35) (layer "F.SilkS") (width 0.09) (tstamp 42cf133c-c7f3-4b68-bc7f-2d7d47dda96c))
  (fp_line (start -59.95 -77.35) (end 59.95 -77.35) (layer "F.SilkS") (width 0.09) (tstamp f69962f1-b28a-4a14-8311-758bea8041a8))
  (fp_line (start -63.3 -82.5) (end -63.5 -82.5) (layer "Dwgs.User") (width 0.12) (tstamp 053bcd06-0eb3-452a-9bd0-305035e71fa8))
  (fp_line (start -60.9 84.75) (end -52.1 83) (layer "Dwgs.User") (width 0.12) (tstamp 23b261f7-4174-4d47-9f83-e912699d93a1))
  (fp_line (start -63.5 83.5) (end -63.5 82.5) (layer "Dwgs.User") (width 0.12) (tstamp 27c9ac35-70ed-415a-8f25-d9cfd188482b))
  (fp_line (start 60 82.5) (end -60 82.5) (layer "Dwgs.User") (width 0.12) (tstamp 2ca5e8ff-641d-4126-8650-97a99d259d2d))
  (fp_line (start -63.5 -82.5) (end -63.5 -83.5) (layer "Dwgs.User") (width 0.12) (tstamp 41111de7-ae27-451d-99ac-3545404f4043))
  (fp_line (start 63.5 83.5) (end 60.9 84.75) (layer "Dwgs.User") (width 0.12) (tstamp 44ba78f6-42e6-4e22-ac5f-d22dc75168c8))
  (fp_line (start -60 -82.5) (end 60 -82.5) (layer "Dwgs.User") (width 0.12) (tstamp 46d95195-9c83-4ecb-9642-572941e1967a))
  (fp_line (start 63.3 -82.5) (end 61.8 -82.5) (layer "Dwgs.User") (width 0.12) (tstamp 48e44dd7-5bae-47c4-b925-c4307b10416a))
  (fp_line (start -63.5 -83.5) (end -60.9 -84.75) (layer "Dwgs.User") (width 0.12) (tstamp 4cd01065-6a78-4ce9-b25f-acb27d15ce12))
  (fp_line (start -60 77.5) (end 60 77.5) (layer "Dwgs.User") (width 0.12) (tstamp 4d94226e-5c3b-4497-a68e-6901d20f3fcd))
  (fp_line (start 60.9 84.75) (end 52.1 83) (layer "Dwgs.User") (width 0.12) (tstamp 4f767ff1-71d6-4759-8db2-bfb0b8245172))
  (fp_line (start 60.9 -84.75) (end 63.5 -83.5) (layer "Dwgs.User") (width 0.12) (tstamp 571561b4-1b2b-43a5-930d-262fdfabf554))
  (fp_line (start 60 82.5) (end 60 -82.5) (layer "Dwgs.User") (width 0.12) (tstamp 62c2e20a-ed1e-4b69-a659-c453b26128f8))
  (fp_line (start -60 -77.5) (end 60 -77.5) (layer "Dwgs.User") (width 0.12) (tstamp 69f8e2ab-0841-45b0-9a53-a683067e459e))
  (fp_line (start -60 82.5) (end -60 -82.5) (layer "Dwgs.User") (width 0.12) (tstamp 7dd770bd-9a0f-49a1-b92d-abcbed7bebfe))
  (fp_line (start 63.5 82.5) (end 63.5 83.5) (layer "Dwgs.User") (width 0.12) (tstamp 7e14f799-5c6a-4813-926b-1a9aca180caa))
  (fp_line (start 63.3 -82.5) (end 63.5 -82.5) (layer "Dwgs.User") (width 0.12) (tstamp 8195cca9-1b45-476f-807f-7f48b5db4647))
  (fp_line (start 63.3 82.5) (end 63.3 -82.5) (layer "Dwgs.User") (width 0.12) (tstamp 8903b686-4a75-4958-80db-d9a4951d93fc))
  (fp_line (start -60.9 -84.75) (end -52.1 -83) (layer "Dwgs.User") (width 0.12) (tstamp 95aa81bf-35aa-4644-99fe-fc3c8da73eda))
  (fp_line (start 63.3 82.5) (end 63.5 82.5) (layer "Dwgs.User") (width 0.12) (tstamp 9902ec92-ed67-4c57-870c-1074a3ff3f69))
  (fp_line (start -63.3 82.5) (end -63.5 82.5) (layer "Dwgs.User") (width 0.12) (tstamp 9e752992-ec03-4489-a4a4-a3e886d50896))
  (fp_line (start 61.8 82.5) (end 63.3 82.5) (layer "Dwgs.User") (width 0.12) (tstamp a2e59c32-a3cc-4568-93b2-757c2b79bce3))
  (fp_line (start -60.9 84.75) (end -63.5 83.5) (layer "Dwgs.User") (width 0.12) (tstamp a60190a7-dd13-4e80-9de4-a152468855b5))
  (fp_line (start -61.8 82.5) (end -61.8 -82.5) (layer "Dwgs.User") (width 0.12) (tstamp abd1080c-438b-47a1-978d-0c0207230db7))
  (fp_line (start -52.1 82.5) (end -52.1 83) (layer "Dwgs.User") (width 0.12) (tstamp ac0154e5-df63-4db1-b2cd-c64c96c75916))
  (fp_line (start 61.8 -82.5) (end 61.8 82.5) (layer "Dwgs.User") (width 0.12) (tstamp aed54fd6-2d1f-4789-8d4c-19f744bc11ac))
  (fp_line (start -63.3 -82.5) (end -63.3 82.5) (layer "Dwgs.User") (width 0.12) (tstamp c8ac214f-13a5-4749-a338-c35975a7b1cf))
  (fp_line (start 52.1 83) (end 52.1 82.5) (layer "Dwgs.User") (width 0.12) (tstamp cc0a2b47-8650-4f30-85aa-9d980d83f5ac))
  (fp_line (start -52.1 -83) (end -52.1 -82.5) (layer "Dwgs.User") (width 0.12) (tstamp ccd52189-2f1e-495c-9038-fcfbbd9645ef))
  (fp_line (start 63.5 -83.5) (end 63.5 -82.5) (layer "Dwgs.User") (width 0.12) (tstamp e1a5fcbc-2e47-4286-9d53-c358cf1fbba2))
  (fp_line (start -63.3 82.5) (end -61.8 82.5) (layer "Dwgs.User") (width 0.12) (tstamp f0ba78ff-5642-4219-a2be-5edfe6f4d28a))
  (fp_line (start -61.8 -82.5) (end -63.3 -82.5) (layer "Dwgs.User") (width 0.12) (tstamp fbd0f165-0cc4-4871-a5e8-17e78d9f05fa))
  (fp_line (start 60.9 -84.75) (end 52.1 -83) (layer "Dwgs.User") (width 0.12) (tstamp fd569132-50c8-44b6-99f2-ec1be4d22a8f))
  (fp_line (start 52.1 -82.5) (end 52.1 -83) (layer "Dwgs.User") (width 0.12) (tstamp ffef2df5-7347-4094-ad77-266e90610245))
  (fp_line (start 60 80) (end 60 -80) (layer "F.Fab") (width 0.1) (tstamp 0650ca61-b84d-4f7b-84fa-f6b1cc0c7147))
  (fp_line (start -60 80) (end 60 80) (layer "F.Fab") (width 0.1) (tstamp 27a4aba1-bfac-4f67-948d-cbad20801c06))
  (fp_line (start -60 -80) (end -60 80) (layer "F.Fab") (width 0.1) (tstamp 794d7e78-1d6c-419f-8fcd-c4707b59e2cc))
  (fp_line (start 60 -80) (end -60 -80) (layer "F.Fab") (width 0.1) (tstamp c932589c-3647-4461-9651-114f418c5f01))
  (fp_line (start 60 -80) (end -60 -80) (layer "F.Fab") (width 0.1) (tstamp ee16dd18-1518-4fd5-9e90-2a2b22c6eaa4))
  (zone (net 0) (net_name "") (layers "B.Paste" "B.Mask" "Margin") (tstamp 01ab4e6c-42da-46ab-9229-64999e2407ff) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour allowed) (footprints not_allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60 77.4)
        (xy -60 77.4)
        (xy -60 73.4)
        (xy 60 73.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layers *.Paste *.Mask "Margin") (tstamp 78b5207f-1554-4827-bf35-c4be2216a7f0) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour allowed) (footprints not_allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60 80)
        (xy -60 80)
        (xy -60 77.4)
        (xy 60 77.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "B.Paste" "B.Mask" "Margin") (tstamp 7908b283-651e-483b-b94b-59b57316694c) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour allowed) (footprints not_allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60 -73.4)
        (xy -60 -73.4)
        (xy -60 -77.4)
        (xy 60 -77.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layers *.Paste *.Mask "Margin") (tstamp 8565a7f9-f09b-46a7-8d6b-78651702a13f) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour allowed) (footprints not_allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60 -77.4)
        (xy -60 -77.4)
        (xy -60 -80)
        (xy 60 -80)
      )
    )
  )
  (model "${ACCELEROMETER_PCB}/Models.3D/1455T1201_Bezel.step"
    (offset (xyz 0 0 42.5))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -90))
  )
  (model "${ACCELEROMETER_PCB}/Models.3D/1455T1201_End_Plate.step"
    (offset (xyz 0 0 42.5))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -90))
  )
  (model "${ACCELEROMETER_PCB}/Models.3D/1455T1201_Extrusion.step"
    (offset (xyz 0 0 -9))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 0 -90))
  )
  (model "${ACCELEROMETER_PCB}/Models.3D/1455T1201_Extrusion_Cap.step"
    (offset (xyz 0 0 -9))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 0 -90))
  )
  (model "${ACCELEROMETER_PCB}/Models.3D/1455T1201_Screws.step"
    (offset (xyz 0 0 42.5))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -90))
  )
)
